| Wireshark 4.7.0 The Wireshark network protocol analyzer

Loading...
Searching...
No Matches
Public Attributes | List of all members
f5eth_tap_data Struct Reference

`#include <packet-f5ethtrailer.h>`

## Public Attributes
uint32_t | magic
uint32_t | trailer_len
uint64_t | flow
uint64_t | peer_flow
char * | virtual_name
uint16_t | slot
uint16_t | tmm
uint8_t | noise_low:1
uint8_t | noise_med:1
uint8_t | noise_high:1
uint8_t | flows_set:1
uint8_t | ingress:2

## Detailed Description

Data structure to hold data returned by the f5ethtrailer tap. Magic has to be first.

## Member Data Documentation

## ◆ flow

uint64_t f5eth_tap_data::flow

Flow ID

## ◆ flows_set

uint8_t f5eth_tap_data::flows_set

If the frame has flow/peerflow fields(1) or not(0)

## ◆ ingress

uint8_t f5eth_tap_data::ingress

Whether the packet was ingress(1), egress(0) or unknown(3)

## ◆ magic

uint32_t f5eth_tap_data::magic

Verify proper version of dissector

## ◆ noise_high

uint8_t f5eth_tap_data::noise_high

If the frame has high noise(1) or not(0)

## ◆ noise_low

uint8_t f5eth_tap_data::noise_low

If the frame has low noise(1) or not(0)

## ◆ noise_med

uint8_t f5eth_tap_data::noise_med

If the frame has medium noise(1) or not(0)

## ◆ peer_flow

uint64_t f5eth_tap_data::peer_flow

Peer Flow ID

## ◆ slot

uint16_t f5eth_tap_data::slot

The slot the handled the packet (F5ETH_TAP_TMM_MAX == unknown)

## ◆ tmm

uint16_t f5eth_tap_data::tmm

The tmm that handled the packet (F5ETH_TAP_sLOT_MAX == unknown)

## ◆ trailer_len

uint32_t f5eth_tap_data::trailer_len

Overall length of the F5 trailer

## ◆ virtual_name

char* f5eth_tap_data::virtual_name

Virtual server name

The documentation for this struct was generated from the following file:

- /builds/wireshark/wireshark/epan/dissectors/packet-f5ethtrailer.h