| Wireshark 4.7.0 The Wireshark network protocol analyzer

Loading...
Searching...
No Matches
Public Attributes | List of all members
DTM_Packet_Downlink_Assignment_t Struct Reference

## Public Attributes
uint8_t | MAC_MODE
uint8_t | RLC_MODE
uint8_t | TIMESLOT_ALLOCATION
Packet_Timing_Advance_t | Packet_Timing_Advance
uint8_t | Exist_P0_and_BTS_PWR_CTRL_MODE
uint8_t | P0
uint8_t | BTS_PWR_CTRL_MODE
uint8_t | PR_MODE
uint8_t | Exist_Power_Control_Parameters
Power_Control_Parameters_t | Power_Control_Parameters
uint8_t | Exist_DOWNLINK_TFI_ASSIGNMENT
uint8_t | DOWNLINK_TFI_ASSIGNMENT
uint8_t | Exist_Measurement_Mapping
Measurement_Mapping_struct_t | Measurement_Mapping
bool | EGPRS_Mode
uint8_t | EGPRS_WindowSize
uint8_t | LINK_QUALITY_MEASUREMENT_MODE
bool | Exist_Packet_Extended_Timing_Advance
uint8_t | Packet_Extended_Timing_Advance

The documentation for this struct was generated from the following file:

- /builds/wireshark/wireshark/epan/dissectors/packet-gsm_rlcmac.h