| Wireshark 4.7.0 The Wireshark network protocol analyzer

Loading...
Searching...
No Matches
Public Attributes | List of all members
NC_MeasurementReport_t Struct Reference

## Public Attributes
uint8_t | NC_MODE
uint8_t | UnionType
union { |
BA_USED_t BA_USED |
uint8_t PSI3_CHANGE_MARK |
} | u |
uint8_t | PMO_USED
uint8_t | SCALE
uint8_t | Exist_ServingCellData
ServingCellData_t | ServingCellData
uint8_t | Count_Repeated_Invalid_BSIC_Info
Repeated_Invalid_BSIC_Info_t | Repeated_Invalid_BSIC_Info [32]
bool | Exist_Repeated_REPORTING_QUANTITY
uint8_t | Count_Repeated_Reporting_Quantity
REPORTING_QUANTITY_t | Repeated_REPORTING_QUANTITY [96]

The documentation for this struct was generated from the following file:

- /builds/wireshark/wireshark/epan/dissectors/packet-gsm_rlcmac.h