| Wireshark 4.7.0 The Wireshark network protocol analyzer

Loading...
Searching...
No Matches
packet-btsdp.h
1/* packet-btsdp.h
2 *
3 * Wireshark - Network traffic analyzer
4 * By Gerald Combs <gerald@wireshark.org>
5 * Copyright 1998 Gerald Combs
6 *
7 * SPDX-License-Identifier: GPL-2.0-or-later
8 */
9
10#ifndef __PACKET_BTSDP_H__
11#define __PACKET_BTSDP_H__
12
13#include "packet-bluetooth.h"
14
15/*
16 * Based on value provided by Bluetooth SIG:
17 * https://www.bluetooth.org/Technical/AssignedNumbers/service_discovery.htm
18 */
19/* protocol UUIDs */
20#define BTSDP_SDP_PROTOCOL_UUID 0x0001
21#define BTSDP_UDP_PROTOCOL_UUID 0x0002
22#define BTSDP_RFCOMM_PROTOCOL_UUID 0x0003
23#define BTSDP_TCP_PROTOCOL_UUID 0x0004
24#define BTSDP_TCS_BIN_PROTOCOL_UUID 0x0005
25#define BTSDP_TCS_AT_PROTOCOL_UUID 0x0006
26#define BTSDP_ATT_PROTOCOL_UUID 0x0007
27#define BTSDP_OBEX_PROTOCOL_UUID 0x0008
28#define BTSDP_IP_PROTOCOL_UUID 0x0009
29#define BTSDP_FTP_PROTOCOL_UUID 0x000A
30#define BTSDP_HTTP_PROTOCOL_UUID 0x000C
31#define BTSDP_WSP_PROTOCOL_UUID 0x000E
32#define BTSDP_BNEP_PROTOCOL_UUID 0x000F
33#define BTSDP_UPNP_PROTOCOL_UUID 0x0010
34#define BTSDP_HIDP_PROTOCOL_UUID 0x0011
35#define BTSDP_HARDCOPY_CONTROL_CHANNEL_PROTOCOL_UUID 0x0012
36#define BTSDP_HARDCOPY_DATA_CHANNEL_PROTOCOL_UUID 0x0014
37#define BTSDP_HARDCOPY_NOTIFICATION_PROTOCOL_UUID 0x0016
38#define BTSDP_AVCTP_PROTOCOL_UUID 0x0017
39#define BTSDP_AVDTP_PROTOCOL_UUID 0x0019
40#define BTSDP_CMTP_PROTOCOL_UUID 0x001B
41#define BTSDP_MCAP_CONTROL_CHANNEL_PROTOCOL_UUID 0x001E
42#define BTSDP_MCAP_DATA_CHANNEL_PROTOCOL_UUID 0x001F
43#define BTSDP_L2CAP_PROTOCOL_UUID 0x0100
44
45/* service UUIDs */
46#define BTSDP_SPP_SERVICE_UUID 0x1101
47#define BTSDP_LAN_SERVICE_UUID 0x1102
48#define BTSDP_DUN_SERVICE_UUID 0x1103
49#define BTSDP_SYNC_SERVICE_UUID 0x1104
50#define BTSDP_OPP_SERVICE_UUID 0x1105
51#define BTSDP_FTP_SERVICE_UUID 0x1106
52#define BTSDP_SYNC_COMMAND_SERVICE_UUID 0x1107
53#define BTSDP_HSP_SERVICE_UUID 0x1108
54#define BTSDP_CTP_SERVICE_UUID 0x1109
55
56#define BTSDP_A2DP_SOURCE_SERVICE_UUID 0x110A
57#define BTSDP_A2DP_SINK_SERVICE_UUID 0x110B
58#define BTSDP_AVRCP_TG_SERVICE_UUID 0x110C
59#define BTSDP_A2DP_DISTRIBUTION_SERVICE_UUID 0x110D
60#define BTSDP_AVRCP_SERVICE_UUID 0x110E
61#define BTSDP_AVRCP_CT_SERVICE_UUID 0x110F
62
63#define BTSDP_ICP_SERVICE_UUID 0x1110
64#define BTSDP_FAX_SERVICE_UUID 0x1111
65#define BTSDP_HSP_GW_SERVICE_UUID 0x1112
66#define BTSDP_WAP_SERVICE_UUID 0x1113
67#define BTSDP_WAP_CLIENT_SERVICE_UUID 0x1114
68
69#define BTSDP_PAN_PANU_SERVICE_UUID 0x1115
70#define BTSDP_PAN_NAP_SERVICE_UUID 0x1116
71#define BTSDP_PAN_GN_SERVICE_UUID 0x1117
72
73#define BTSDP_BPP_DIRECT_PRINTING_SERVICE_UUID 0x1118
74#define BTSDP_BPP_REFERENCE_PRINTING_SERVICE_UUID 0x1119
75
76#define BTSDP_BIP_SERVICE_UUID 0x111A
77#define BTSDP_BIP_RESPONDER_SERVICE_UUID 0x111B
78#define BTSDP_BIP_AUTO_ARCH_SERVICE_UUID 0x111C
79#define BTSDP_BIP_REF_OBJ_SERVICE_UUID 0x111D
80
81#define BTSDP_HFP_SERVICE_UUID 0x111E
82#define BTSDP_HFP_GW_SERVICE_UUID 0x111F
83
84#define BTSDP_BPP_DIRECT_PRINTING_REF_OBJ_SERVICE_UUID 0x1120
85#define BTSDP_BPP_REFLECTED_UI_SERVICE_UUID 0x1121
86#define BTSDP_BPP_SERVICE_UUID 0x1122
87#define BTSDP_BPP_STATUS_SERVICE_UUID 0x1123
88
89#define BTSDP_HID_SERVICE_UUID 0x1124
90
91#define BTSDP_HCRP_SERVICE_UUID 0x1125
92#define BTSDP_HCRP_PRINT_SERVICE_UUID 0x1126
93#define BTSDP_HCRP_SCAN_SERVICE_UUID 0x1127
94
95#define BTSDP_CIP_SERVICE_UUID 0x1128
96
97#define BTSDP_VIDEO_CONFERENCING_GW_SERVICE_UUID 0x1129 /* not assigned*/
98
99#define BTSDP_UDI_MT_SERVICE_UUID 0x112A /* not assigned*/
100#define BTSDP_UDI_TA_SERVICE_UUID 0x112B /* not assigned*/
101
102#define BTSDP_AUDIO_VIDEO_SERVICE_UUID 0x112C /* not assigned*/
103
104#define BTSDP_SAP_SERVICE_UUID 0x112D
105
106#define BTSDP_PBAP_PCE_SERVICE_UUID 0x112E
107#define BTSDP_PBAP_PSE_SERVICE_UUID 0x112F
108#define BTSDP_PBAP_SERVICE_UUID 0x1130
109
110#define BTSDP_HSP_HS_SERVICE_UUID 0x1131
111
112#define BTSDP_MAP_ACCESS_SRV_SERVICE_UUID 0x1132
113#define BTSDP_MAP_NOTIFICATION_SRV_SERVICE_UUID 0x1133
114#define BTSDP_MAP_SERVICE_UUID 0x1134
115
116#define BTSDP_GNSS_UUID 0x1135
117#define BTSDP_GNSS_SERVER_UUID 0x1136
118
119#define BTSDP_3D_DISPLAY_UUID 0x1137
120#define BTSDP_3D_GLASSES_UUID 0x1138
121#define BTSDP_3D_SYNCHRONIZATION_UUID 0x1139
122
123#define BTSDP_MULTI_PROFILE_UUID 0x113A
124#define BTSDP_MULTI_PROFILE_SC_UUID 0x113B
125
126#define BTSDP_CTN_ACCESS_SERVICE_UUID 0x113C
127#define BTSDP_CTN_NOTIFICATION_SERVICE_UUID 0x113D
128#define BTSDP_CTN_SERVICE_UUID 0x113E
129
130#define BTSDP_DID_SERVICE_UUID 0x1200
131
132#define BTSDP_GENERIC_NETWORKING_SERVICE_UUID 0x1201
133#define BTSDP_GENERIC_FILE_TRANSFER_SERVICE_UUID 0x1202
134#define BTSDP_GENERIC_AUDIO_SERVICE_UUID 0x1203
135#define BTSDP_GENERIC_TELEPHONY_SERVICE_UUID 0x1204
136
137#define BTSDP_ESDP_UPNP_SERVICE_SERVICE_UUID 0x1205
138#define BTSDP_ESDP_UPNP_IP_SERVICE_SERVICE_UUID 0x1206
139#define BTSDP_ESDP_UPNP_IP_PAN_SERVICE_UUID 0x1300
140#define BTSDP_ESDP_UPNP_IP_LAP_SERVICE_UUID 0x1301
141#define BTSDP_ESDP_UPNP_L2CAP_SERVICE_UUID 0x1302
142
143#define BTSDP_VDP_SOURCE_SERVICE_UUID 0x1303
144#define BTSDP_VDP_SINK_SERVICE_UUID 0x1304
145#define BTSDP_VDP_DISTRIBUTION_SERVICE_UUID 0x1305
146
147#define BTSDP_HDP_SERVICE_UUID 0x1400
148#define BTSDP_HDP_SOURCE_SERVICE_UUID 0x1401
149#define BTSDP_HDP_SINK_SERVICE_UUID 0x1402
150
151#define BTSDP_LOCAL_SERVICE_FLAG_MASK 0x0001
152#define BTSDP_SECONDARY_CHANNEL_FLAG_MASK 0x0002
153
154#define SDP_PSM_DEFAULT 1
155
156/* This structure is passed to other dissectors
157 * and contains information about the relation between service, PSM/server
158 * channel, local/remote service. The btrfcomm and btl2cap dissectors
159 * need this information to determine the kind of data transferred on
160 * dynamically assigned server channels and PSM's, respectively.
161 */
162 typedef struct _btsdp_data_t {
163 uint32_t interface_id;
164 uint32_t adapter_id;
165 uint32_t chandle;
166 uint32_t frame_number;
167 uint32_t service; /* service UUID, see below */
168 uint32_t channel; /* rfcomm server channel or PSM */
169 uint16_t protocol; /* either rfcomm or l2cap UUID */
170 uint16_t flags; /* indicate if the service is local or remote
171 peer device) and/or a secondary PSM */
172} btsdp_data_t;
173
174
175 typedef struct _service_info_t {
176 uint32_t interface_id;
177 uint32_t adapter_id;
178 uint32_t sdp_psm;
179 uint32_t direction;
180 uint32_t bd_addr_oui;
181 uint32_t bd_addr_id;
182 uint32_t type;
183 uint32_t channel;
184
185 bluetooth_uuid_t uuid;
186 int protocol_order; /* main service protocol has 0, goep -1, additional protocol 1, 2... */
187 int protocol;
188
189 void *data; /* Used to transfer service record data to profiles */
190
191 struct _service_info_t *parent_info;
192} service_info_t;
193
194 extern const value_string hid_country_code_vals[];
195
196 extern service_info_t* btsdp_get_service_info(wmem_tree_key_t* key);
197
198#endif
199
200/*
201 * Editor modelines - https://www.wireshark.org/tools/modelines.html
202 *
203 * Local variables:
204 * c-basic-offset: 4
205 * tab-width: 8
206 * indent-tabs-mode: nil
207 * End:
208 *
209 * vi: set shiftwidth=4 tabstop=8 expandtab:
210 * :indentSize=4:tabSize=8:noTabs=true:
211 */
_btsdp_data_t
Definition packet-btsdp.h:162
_service_info_t
Definition packet-btsdp.h:175
_uuid_t
Definition packet-bluetooth.h:195
_value_string
Mapping between a 32-bit integer value and its string representation.
Definition value_string.h:33
_wmem_tree_key_t
Represents a key used in a wmem tree.
Definition wmem_tree.h:297